Jazz Medicine Cabinet 80 - Installation Manual

Preliminary Instructions:

Before you begin assembling and installing the furniture, read all the instructions carefully.

Assembly and installation of the product must be performed on a clean and flat surface. We recommend hiring professionals to perform hydraulic and electrical installations.

To install this product, you will need:

Two people Phillips screwdriver Bubble level Tape measure Drill Hammer Rubber mallet

Jazz Set 80

Additional Information:

To clean the cabinet and the washbasin, use a soft, moist cloth (with water). Then use a dry cloth.

The furniture is resistant to water splashes and the natural humidity of the bathroom.

After installing the product, check if the hydraulic devices are leaking. If there is a leakage, contact a plumber to solve the problem.

Excessive water can damage the product.

1. Insert the plastic anchors in the wall, in the points where the mirror will be hanged. These points are given by the metallic hardware already installed on the mirror. Look at drilling position “**C**” in the drilling manual. Insert the 4x40 screws in the anchors, leaving 2mm of the screw head out. The medicine cabinet possesses metallic hardware already installed for hanging.

In the hardware kit you will find:

2 Screws 4x40 2 Plastic Anchors