Malta Cabinet - Installation Manual

Preliminary Instructions:

Before you begin assembling and installing the furniture, read all the instructions carefully.

Assembly and installation of the product must be performed on a clean and flat surface. We recommend hiring professionals to perform hydraulic and electrical installations.

To install this product, you will need:

Two people Phillips screwdriver Bubble level Tape measure Drill Hammer Rubber mallet

Additional Information:

To clean the cabinet and the washbasin, use a soft, moist cloth (with water). Then use a dry cloth.

The furniture is resistant to water splashes and the natural humidity of the bathroom.

After installing the product, check if the hydraulic devices are leaking. If there is a leakage, contact a plumber to solve the problem.

Excessive water can damage the product.

Malta Set 60

5. Install the handle with the 3,5x14 screws.

4. Place the basin on the cabinet.

3. If you need to remove the drawers to perform any installations, pull the drawer out and release the side locks as shown in the figure below. The left lock should be pushed up while the right lock should be pushed down. After releasing the slides, simply pull the drawers.

2. Insert the 6x50 screws through the metallic hardware from the inside of the cabinet, securing the cabinet to the wall with the anchors.

1. Insert the plastic anchors in the wall, in the points where the furniture will be hanged. These points are given by the metallic hardware inside the cabinet. Install the cabinet at a comfortable height.

In the hardware kit you will find:

3,5x14 screws Handle Plastic Anchors 6x50 screws Plastic covers